The requested changes are as follows:

**P. 13, Figure 10:**

The unit for panels (g-i) and (j-l) should be [mmol m-3].

Explanation: The unit for PO4 and AOU is wrong in panels (g-i). The correct unit is [mmol m-3].

**P. 22, Fig. B2:**

Please change the unit for the y-axis to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 24, Fig. B7:**

Please change the unit of y-axis to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 25, Fig. B8:**

Please change the unit of y-axis for panels (d-g) to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 28, Fig. C4:**

Please change the unit of y-axis for panels (b-d) to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 28, Fig. C5:**

Please change the unit of y-axis for panels (b-d) to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 29, Fig. C6:**

Please change the unit of y-axis for panels (b-d) to:

Depth (km)

Explanation: The unit for the vertical axis is wrong. The depth unit should be (km), not (m).

**P. 29, caption of Fig. C7:**

Please change to:

from 1960 to 2009.

Explanation: There is a mistake in the caption. The figure is for the period from 1960 to 2009 (see text in Page 8 Line7), not for pre-industrial to 1990s.