The files listed below are animations of CFE images
in three lighting modes after processiong. To reduce file size, 
The pixel resolution of these animations is approximately 26 µm. 
In other words, 2 times degraded compared to original images.  

NH1204_CFE001_ATN_160.mov
NH1204_CFE001_DRK_160.mov
NH1204_CFE001_PL2_60.mov
NH1204_CFE001_TRA.mov
NH1301_BUOY84_ATN_160.mov
NH1301_BUOY84_DRK_160.mov
NH1301_BUOY84_PL2_60.mov
NH1301_BUOY84_TRA.mov
NH1301_CFE001_ATN_160.mov
NH1301_CFE001_DRK_160.mov
NH1301_CFE001_PL2_60.mov
NH1301_CFE001_TRA.mov
NH1304_CFE001_ATN_160.mov
NH1304_CFE001_DRK_160.mov
NH1304_CFE001_PL2_60.mov
NH1304_CFE001_TRA.mov

TRA - Transmitted Light - in counts
ATN - Calculated as log10 of transmission
      image intensity scaled so that 160 counts = 255
DRK - Dark Field Counts
      inage intensity scaled so that 160 counts = 255
PL2 - CrossPolarized Transmitted light
      image intensity scaled so that  60 counts = 255. 

The first 6 letters designate the research vessel and cruise number. 
NH stands for R/V New Horison
1204 May/June 2012
1301 Jan 2013
1304 Mar 2013

The next 6 letters after the _ indicate CFE001 or BUOY84 as 
from the Carbon FLux Explorer or from BUOY_OSR, respectively
=====================================
The following figures are full resolution images
after processing to Attenuance. A count of 100
corresponds to an Attenuance value of 1.0

20130120_1049_CFE001_ATNc.bmp
20130120_1111_CFE001_ATNr.bmp
20130120_1130_CFE001_ATNr.bmp
20130120_1155_CFE001_ATNr.bmp
20130120_1217_CFE001_ATNr.bmp
20130120_1239_CFE001_ATNr.bmp
====================================
NH1301SatImages.pptx remote sensing images of chlorophyll 
for NH1301. 

20160221_Summary_CFE_Fluxes_BiogeosciencesSuppl.Excel.xlsx
Contains data used for calculations of flux. 

